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Technical data
Mercedes-Maybach S 680 Saloon
As of: 08 April 2026


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	V8

	Displacement
	cc  
	3,982

	Hub x bore
	mm x mm  
	92.00 x 83.00

	Rated output1
	kW [hp] at rpm  
	450 [612]/5,500-6,100

	Rated torque2
	Nm at rpm  
	850/2,500-4,500

	Compression ratio
	  
	10.50 : 1

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)3
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 390

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Ratios (1/2/3/4/5/6/7/8/9/R1)
	  
	5,35/3,24/2,25/1,64/1,21/1,00/0,87/0,72/0,60/R1 4,80

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,484/1,921/1,510

	Wheelbase
	mm  
	3,396

	Turning circle
	m  
	12.40

	Track width, front/rear
	mm  
	1,655/1,683

	Luggage compartment capacity, VDA4
	l  
	480

	Kerb weight/payload/permissible gross mass5
	kg  
	2,430

	Tank capacity/reserve
	l  
	76/8

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.0

	Top speed
	km/h  
	250

	Energy consumption (combined)6
	l/100 km  
	11.7 - 11.0

	CO₂ emissions (combined)6
	g/km  
	267 - 252

	CO₂ class6
	  
	G 



1 The specified rated power corresponds to the continuously available engine output defined in accordance with DIN 70020, ISO 14396 and ECE Regulation No. 24 under standardised test conditions. The power output is reproducible under standardised temperature, load and ambient conditions and represents the continuously available power output of the combustion engine.
2 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
3 The specified maximum power describes the peak power of the electric drive that is briefly available under the test conditions of ECE Regulation No. 85. This peak power is only available for limited periods and may vary depending on temperature, charge, conditioning and environmental conditions. The actual available power may differ from the specified maximum value depending on operating conditions.
4 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
5 Kerb weight, ready-to-drive in accordance with EU.
6 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com.
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