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Technical Data
Mercedes-Benz S 350 d 4MATIC Saloon, long version 
As of: 18 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,989

	Rated output1
	kW [hp] at rpm  
	230 [313]/3600 - 4800

	Rated torque1
	Nm at rpm  
	650/1200 - 3200

	Fuel mix preparation
	 
	Injection pump/injection system model: 2-plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 320

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8 J x 18 ET 29.0 / 8 J x 18 ET 29.0

	Tyres, front/rear
	  
	235/55 R18 / 235/55 R18

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,304/1,921/1,503

	Wheelbase
	mm  
	3,216

	Turning circle
	m  
	11.90

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	510

	Kerb weight/payload/permissible gross mass3
	kg  
	2,250

	Tank capacity/reserve
	l  
	76/8

	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100




	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	5.4

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	6.9 - 6.2

	CO₂ emissions (combined)4
	g/km  
	182 - 163

	CO₂ class4
	  
	G - F



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 





Technical Data
Mercedes-Benz S 350 d 4MATIC Saloon 
As of: 18 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,989

	Rated output1
	kW [hp] at rpm  
	230 [313]/3600 - 4800

	Rated torque1
	Nm at rpm  
	650/1200 - 3200

	Fuel mix preparation
	 
	Injection pump/injection system model: 2-plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 320

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8 J x 18 ET 29.0 / 8 J x 18 ET 29.0

	Tyres, front/rear
	  
	235/55 R18 / 235/55 R18

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,194/1,921/1,503

	Wheelbase
	mm  
	3,106

	Turning circle
	m  
	11.60

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	510

	Kerb weight/payload/permissible gross mass3
	kg  
	2,230

	Tank capacity/reserve
	l  
	76/8




	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	5.4

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	6.8 - 6.2

	CO₂ emissions (combined)4
	g/km  
	179 - 162

	CO₂ class4
	  
	G - F



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 450 4MATIC Saloon, long version 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	280 [381]/5.000 - 6.100

	Rated torque1
	Nm at rpm  
	560/2000 - 4500


	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 320

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8 J x 18 ET 29.0 / 8 J x 18 ET 29.0

	Tyres, front/rear
	  
	235/55 R18 / 235/55 R18

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,304/1,954/1,503

	Wheelbase
	mm  
	3,216

	Turning circle
	m  
	11.90

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	530

	Kerb weight/payload/permissible gross mass3
	kg  
	2,185

	Tank capacity/reserve
	l  
	76/8

	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.9

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	9.0 - 8.2

	CO₂ emissions (combined)4
	g/km  
	206 - 186

	CO₂ class4
	  
	G 



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 450 4MATIC Saloon 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	280 [381]/5.000 - 6.100

	Rated torque1
	Nm at rpm  
	560/2000 - 4500

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 320

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8 J x 18 ET 29.0 / 8 J x 18 ET 29.0

	Tyres, front/rear
	  
	235/55 R18 / 235/55 R18

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,194/1,921/1,503

	Wheelbase
	mm  
	3,106

	Turning circle
	m  
	11.60

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	530

	Kerb weight/payload/permissible gross mass3
	kg  
	2,165

	Tank capacity/reserve
	l  
	76/8

	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.9

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	8.9 - 8.1

	CO₂ emissions (combined)4
	g/km  
	203 - 185

	CO₂ class4
	  
	G 



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 450 d 4MATIC Saloon, long version 
As of: 18 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,989

	Rated output1
	kW [hp] at rpm  
	270 [367]/4000 - 4000

	Rated torque1
	Nm at rpm  
	750/1350 - 2800

	Fuel mix preparation
	 
	Injection pump/injection system model: 2-plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 320

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,304/1,921/1,503

	Wheelbase
	mm  
	3,216

	Turning circle
	m  
	11.90

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	510

	Kerb weight/payload/permissible gross mass3
	kg  
	2,255

	Tank capacity/reserve
	l  
	76/8




	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	5.1

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	6.9 - 6.3

	CO₂ emissions (combined)4
	g/km  
	182 - 165

	CO₂ class4
	  
	G - F



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 450 d 4MATIC Saloon 
As of: 18 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,989

	Rated output1
	kW [hp] at rpm  
	270 [367]/4,000

	Rated torque1
	Nm at rpm  
	750/1,350 – 2,800

	Fuel mix preparation
	 
	Injection pump/injection system model: 2-plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 320

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,194/1,921/1,503

	Wheelbase
	mm  
	3,106

	Turning circle
	m  
	11.60

	Track width, front/rear
	mm  
	1,660/1,683

	Luggage compartment capacity, VDA2
	l  
	510

	Kerb weight/payload/permissible gross mass3
	kg  
	2,235

	Tank capacity/reserve
	l  
	76/8




	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	5.1

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	6.9 - 6.3

	CO₂ emissions (combined)4
	g/km  
	179 - 164

	CO₂ class4
	  
	G - F



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 450 e Saloon with EQ Hybrid technology, long version 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x2 (RWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	240 [326]/4,250 – 6,100

	Rated torque1
	Nm at rpm  
	540/2,200 – 4,250

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	120 [163]

	Rated torque (peak) (electric)
	Nm  
	480

	Rated output system output
	kW [hp]  
	320 [435]

	System torque
	Nm  
	680

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,304/1,921/1,503

	Wheelbase
	mm  
	3,216

	Turning circle
	m  
	11.70

	Track width, front/rear
	mm  
	1,655/1,651

	Luggage compartment capacity, VDA2
	l  
	345




	Kerb weight/payload/permissible gross mass3
	kg  
	2,465

	Tank capacity/reserve
	l  
	67/8

	HV battery - usable energy content
	kWh  
	21.96

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	5.7

	Top speed
	km/h  
	250

	Energy consumption (weighted, combined)4
	kWh/100km  
plus l/100 km  
	18.0-16.6
3.1 - 2.2

	Fuel consumption with discharged battery (combined)4
	l/100 km  
	8.7 - 7.5

	CO₂ emissions (weighted, combined)4
	g/km  
	71 - 51

	CO₂ class4
	

	B / G – F

	Electric range (EAER)4
	km  
	95 – 117



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 Figures are preliminary and were determined internally in accordance with the “WLTP test procedure” certification method. At present, there has been neither an EC type approval nor a certificate of conformity with official values. There may be discrepancies between the figures provided and the official values. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 450 e Saloon with EQ Hybrid technology 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x2 (RWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	240 [326]/4,250 – 6,100

	Rated torque1
	Nm at rpm  
	540/2,200 – 4,250

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	120 [163]

	Rated torque (peak) (electric)
	Nm  
	480

	Rated output system output
	kW [hp]  
	320 [435]

	System torque
	Nm  
	680

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,194/1,921/1,503

	Wheelbase
	mm  
	3,106

	Turning circle
	m  
	11.40

	Track width, front/rear
	mm  
	1,655/1,651

	Luggage compartment capacity, VDA2
	l  
	345




	Kerb weight/payload/permissible gross mass3
	kg  
	2,445

	Tank capacity/reserve
	l  
	67/8

	HV battery - usable energy content
	kWh  
	21.96

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	5.7

	Top speed
	km/h  
	250

	Energy consumption (weighted, combined)4
	kWh/100km  
plus l/100 km  
	17.8-16.5
2.9 – 2.1

	Fuel consumption with discharged battery (combined)4
	l/100 km  
	8.6 - 7.4

	CO₂ emissions (weighted, combined)4
	g/km  
	69 - 50

	CO₂ class4
	

	B / G - F

	Electric range (EAER)4
	km  
	96 - 118



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 Figures are preliminary and were determined internally in accordance with the “WLTP test procedure” certification method. At present, there has been neither an EC type approval nor a certificate of conformity with official values. There may be discrepancies between the figures provided and the official values. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 500 4MATIC Saloon, long version 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	330 [449]/5,500 – 6,100

	Rated torque1
	Nm at rpm  
	600/2,200 – 5,000

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,304/1,921/1,503

	Wheelbase
	mm  
	3,216

	Turning circle
	m  
	11.90

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	530

	Kerb weight/payload/permissible gross mass3
	kg  
	2,195

	Tank capacity/reserve
	l  
	76/8

	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.5

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	9.1 - 8.3

	CO₂ emissions (combined)4
	g/km  
	206 - 188

	CO₂ class4
	  
	G 



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 500 4MATIC Saloon 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	330 [449]/5,500 – 6,100

	Rated torque1
	Nm at rpm  
	600/2,200 – 5,000

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,194/1,921/1,503

	Wheelbase
	mm  
	3,106

	Turning circle
	m  
	11.60

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	530

	Kerb weight/payload/permissible gross mass3
	kg  
	2,175

	Tank capacity/reserve
	l  
	76/8

	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.5

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	8.9 - 8.2

	CO₂ emissions (combined)4
	g/km  
	203 - 187

	CO₂ class4
	  
	G 



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 The stated figures were determined in accordance with the prescribed WLTP (Worldwide harmonised Light vehicles Test Procedures) measuring process. The specified ranges refer to the European market. The energy consumption and CO₂ emissions of a passenger car depend not only on the efficient utilisation of the fuel or energy source by the vehicle, but also on the driving style and other non-technical factors. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 580 4MATIC Saloon, long version 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	V8

	Displacement
	cc  
	3,982

	Hub x bore
	mm x mm  
	92.0 x 83.0

	Rated output1
	kW [hp] at rpm  
	395 [537]/5.500 - 6.100

	Rated torque1
	Nm at rpm  
	750/2.500 – 4.500

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,304/1,921/1,503

	Wheelbase
	mm  
	3,216

	Turning circle
	m  
	11.90

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	530

	Kerb weight/payload/permissible gross mass3
	kg  
	2,270

	Tank capacity/reserve
	l  
	76/8

	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.0

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	11.3 - 10.6

	CO₂ emissions (combined)4
	g/km  
	258 - 241

	CO₂ class4
	  
	G 



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 Figures are preliminary and were determined internally in accordance with the “WLTP test procedure” certification method. At present, there has been neither an EC type approval nor a certificate of conformity with official values. There may be discrepancies between the figures provided and the official values. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 580 4MATIC Saloon
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	V8

	Displacement
	cc  
	3,982

	Hub x bore
	mm x mm  
	92.0 x 83.0

	Rated output1
	kW [hp] at rpm  
	395 [537]/5,500 – 6,100

	Rated torque1
	Nm at rpm  
	750/2,500 – 4,500

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	17 [23]

	Rated torque (peak) (electric)
	Nm  
	205

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,194/1,921/1,503

	Wheelbase
	mm  
	3,106

	Turning circle
	m  
	11.60

	Track width, front/rear
	mm  
	1,660/1,688

	Luggage compartment capacity, VDA2
	l  
	530

	Kerb weight/payload/permissible gross mass3
	kg  
	2,250

	Tank capacity/reserve
	l  
	76/8

	Permissible trailer load, unbraked, braked [at 12%]
	kg  
	750/2,100

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.0

	Top speed
	km/h  
	250

	Energy consumption (combined)4
	l/100 km  
	11.2-10.5

	CO₂ emissions (combined)4
	g/km  
	256 - 240

	CO₂ class4
	  
	G 



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 Figures are preliminary and were determined internally in accordance with the “WLTP test procedure” certification method. At present, there has been neither an EC type approval nor a certificate of conformity with official values. There may be discrepancies between the figures provided and the official values. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com. 






Technical Data
Mercedes-Benz S 580 e 4MATIC Saloon with EQ Hybrid technology, long version 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	330 [449]/5.500 - 6.100

	Rated torque1
	Nm at rpm  
	560/2.200 – 5.000

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	120 [163]

	Rated torque (peak) (electric)
	Nm  
	480

	Rated output system output
	kW [hp]  
	430 [585]

	System torque
	Nm  
	750

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,304/1,921/1,503

	Wheelbase
	mm  
	3,216

	Turning circle
	m  
	11.90

	Track width, front/rear
	mm  
	1,655/1,683

	Luggage compartment capacity, VDA2
	l  
	345




	Kerb weight/payload/permissible gross mass3
	kg  
	2,515

	Tank capacity/reserve
	l  
	67/8

	HV battery - usable energy content
	kWh  
	21.96

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.4

	Top speed
	km/h  
	250

	Energy consumption (weighted, combined)4
	kWh/100km  
plus l/100 km  
	18.2–17.0
3.0-2.6

	Fuel consumption with discharged battery (combined)4
	l/100 km  
	8.8–8.1

	CO₂ emissions (weighted, combined)4
	g/km  
	73–61

	CO₂ class4
	

	B/G

	Electric range (EAER)4
	km  
	92-103



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 Figures are preliminary and were determined internally in accordance with the “WLTP test procedure” certification method. At present, there has been neither an EC type approval nor a certificate of conformity with official values. There may be discrepancies between the figures provided and the official values. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com.






Technical Data
Mercedes-Benz S 580 e 4MATIC Saloon with EQ Hybrid technology 
As of: 11 December 2025


	Engine, drive system and battery

	Drive system
	  
	4x4 (AWD)

	Cylinder arrangement/number
	  
	L6

	Displacement
	cc  
	2,999

	Hub x bore
	mm x mm  
	92.4 x 83.0

	Rated output1
	kW [hp] at rpm  
	330 [449]/5.500 - 6.100

	Rated torque1
	Nm at rpm  
	560/2200 - 5000

	Fuel mix preparation
	 
	Injection pump/injection system model: Single plunger pump

	Rated power (peak) (electric)
	kW [hp]  
	120 [163]

	Rated torque (peak) (electric)
	Nm  
	480

	Rated output system output
	kW [hp]  
	430 [585]

	System torque
	Nm  
	750

	Suspension and steering

	Front axle
	 
	Front springs: Air spring

	Rear axle
	 
	Rear springs: Air spring

	Front brakes
	
mm  
	Brake type: Discs, internally ventilated and perforated
Disc or drum diameter: 370

	Rear brakes
	
mm  
	Brake type: Discs, internally ventilated
Disc or drum diameter: 360

	Steering
	 
	Power steering: Speed-dependent, electro-mechanical

	Rims, front/rear
	  
	8,5 J x 19 ET 31.5 / 8,5 J x 19 ET 31.5

	Tyres, front/rear
	  
	255/45 R19 / 255/45 R19

	Dimensions and weights

	Number of doors/seats
	  
	4/5

	Length/width/height
	mm  
	5,194/1,921/1,503

	Wheelbase
	mm  
	3,106

	Turning circle
	m  
	11.60

	Track width, front/rear
	mm  
	1,655/1,651

	Luggage compartment capacity, VDA2
	l  
	345




	Kerb weight/payload/permissible gross mass3
	kg  
	2,495

	Tank capacity/reserve
	l  
	67/8

	HV battery - usable energy content
	kWh  
	21.96

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s  
	4.4

	Top speed
	km/h  
	250

	Energy consumption (weighted, combined)4
	kWh/100km  
plus l/100 km  
	18.1–16.9
3.0-2.6

	Fuel consumption with discharged battery (combined)4
	l/100 km  
	8.7–8.0

	CO₂ emissions (weighted, combined)4
	g/km  
	71–60

	CO₂ class4
	

	B/G

	Electric range (EAER)4
	km  
	93-103



1 Figures for rated output and rated torque according to Regulation (EC) No. 595/2009 or Regulation (EC) No. 715/2007 in the currently applicable version.
2 according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment
3 Kerb weight, ready-to-drive in accordance with EU.
4 Figures are preliminary and were determined internally in accordance with the “WLTP test procedure” certification method. At present, there has been neither an EC type approval nor a certificate of conformity with official values. There may be discrepancies between the figures provided and the official values. Further information on the vehicles on offer, including the WLTP values, can be found on a country-specific basis at https://www.mercedes-benz.com.
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