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Dati tecnici
Aggiornamento: 6 agosto 2026
I nuovi modelli Mercedes-Benz Classe C Berlina

	Mercedes-Benz C-Class Saloon with high-tech petrol engine 2x4 (RWD)


	
	
	C 200
	C 250
	C 300
	C 300 e

	Drive
	

	Cylinder arrangement/number
	
	I4
	I4
	I4
	I4

	Displacement
	cc
	1,999
	1,999
	1,999
	1,999

	Rated output
	kW/hp
	130/177
	160/218
	190/258
	160/218

	at
	rpm
	5,000-6,100
	5,000-6,100
	5,800-5,800
	5,000-6,100

	Rated torque 
	Nm
	250
	320
	400
	320

	at
	rpm
	1,400-4,000
	1,400-4,000
	2,000-3,200
	1,800-4,000

	Electric motor power (peak)
	kW
	17
	17
	17
	100

	Electric motor torque (peak)
	Nm
	205
	205
	205
	440

	Dimensions and weights

	Length/width/height
	mm
	4,766/1,820/1,438
	4,766/1,820/1,438
	4,766/1,820/1,438
	4,766/1,820/1,442

	Wheelbase
	mm
	2,865
	2,865
	2,865
	2,865

	Turning circle
	m
	11.07
	11.07
	11.07
	11.07

	Track width front/rear
	mm
	1,582/1,594
	1,582/1,594
	1,582/1,594
	1,579/1,583

	Luggage compartment capacity, VDA[endnoteRef:1] [1:  according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment] 

	l
	455
	455
	455
	315

	Kerb weight/payload/
permissible gross mass
	kg
	1,705/545/2,250
	1,725/540/2,265
	1,760/520/2,280
	2,095/520/2,615

	Tank capacity/reserve
	l
	66/7
	66/7
	66/7
	50/7

	Permissible trailer load, unbraked, braked (at 12%)
	kg
	750/1,800
	750/1,800
	750/1,800
	750/1,800

	Performance
	
	
	

	Acceleration 0–100 km/h
	s
	8.5
	7.3
	6.1
	5.9

	Top speed
	km/h
	232
	248
	250
	240

	Fuel consumption and emissions

	Energy consumption combined, weighted (*with discharged battery)/ energy consumption combined, weighted + fuel consumption combined, weighted [endnoteRef:2] [2:  The specified values were determined in accordance with the prescribed measurement procedure WLTP (Worldwide harmonised Light-duty vehicles Test Procedures). The energy consumption and CO2 emissions of a passenger car depend not only on the efficient utilisation of fuel or the respective energy carrier by the car, but also on the driving style and other non-technical factors.] 

	l/100 km/


kw/h
l/100 km
	6.8-6.2
	6.9-6.2
	7.0-6.3
	*7.5-6.8


15.9-15.0
+2.6-2.3

	CO2 emissions combined, weighted/ CO2 emissions discharged battery2 
	g/km
	156-141
	156-141
	159-144
	59-52/
172-154

	CO2 class/ CO2 class discharged battery2
	
	F-E
	F-E
	F-E
	B/F-E

	Prices

	Price (excl. VAT)[endnoteRef:3] [3:  Purchase price in Germany excluding VAT, plus delivery costs or costs for factory collection.] 

	euros
	41,045
	46,045
	50,655
	56,005

	Price (incl. VAT)[endnoteRef:4] [4:  Purchase price in Germany including VAT, excluding delivery costs or factory collection costs.] 

	euros
	48,844
	54,794
	60,279
	66,646





	Mercedes-Benz C-Class Saloon with high-tech petrol engine 4x4 (AWD)

	

	
	
	C 250 4MATIC 
	C 300 e 4MATIC
	C 400 e 4MATIC

	Drive
	
	

	Cylinder arrangement/number
	
	I4
	I4
	I4

	Displacement
	cc
	1,999
	1,999
	1,999

	Rated output
	kW/hp
	160/218
	160/218
	190/258

	at
	rpm
	5,000-6,100
	5,000-6,100
	5,800-5,800

	Rated torque 
	Nm
	320
	320
	400

	at
	rpm
	1,400-4,000
	1,800-4,000
	2,000-3,200

	Electric motor power (peak)
	kW
	17
	100
	100

	Electric motor torque (peak)
	Nm
	205
	440
	440

	Dimensions and weights

	Length/width/height
	mm
	4,766/1,820/1,438
	4,766/1,820/1,442
	4,766/1,820/1,442

	Wheelbase
	mm
	2,865
	2,865
	2,865

	Turning circle
	m
	11.45
	11.45
	11.45

	Track width front/rear
	mm
	1,582/1,594
	1,581/1,583
	1,581/1,583

	Luggage compartment capacity, VDA1
	l
	455
	315
	315

	Kerb weight/payload/
permissible gross mass
	kg
	1,785/535/
2,320
	2,140/530/2,670
	2,140/530/2,670

	Tank capacity/reserve
	l
	66/7
	50/7
	50/7

	Permissible trailer load, unbraked, braked (at 12%)
	kg
	750/1,800
	750/1,800
	750/1,800

	Performance
	
	

	Acceleration 0–100 km/h
	s
	7.1
	6.1
	5.3

	Top speed
	km/h
	246
	240
	240

	Fuel consumption and emissions

	Energy consumption combined, weighted (*with discharged battery)/ energy consumption combined, weighted + fuel consumption combined, weighted2
	l/100 km/


kw/h/
l/100 km
	7.2-6.3
	*7.8-6.9


16.4-15.8
+2.8-2.1
	*7.8-6.9


16.4-15.8
+2.8-2.1

	CO2 emissions combined, weighted/ CO2 emissions discharged battery2
	g/km
	164-145
	64-48/
178-156
	64-48/
178-156

	CO2 class combined, weighted/ CO2 class discharged battery2
	
	F-E
	B/G-F
	B/G-F

	Prices

	Price (excl. VAT)3
	euros
	48,045
	58,005
	61,805

	Price (incl. VAT)4
	euros
	57,174
	69,026
	73,548




	Mercedes-Benz C-Class Saloon with high-tech diesel engine


	
	
	C 200 d
	C 250 d
	C 250 d 4MATIC


	Drive
	
	


	Cylinder arrangement/number
	
	I4
	I4
	I4

	Displacement
	cc
	1,992
	1,992
	1,992

	Rated output
	kW/hp
	120/163
	147/200
	147/200

	at
	rpm
	3,200-4,400
	3,400-3,600
	3,400-3,600

	Rated torque 
	Nm
	380
	440
	440

	at
	rpm
	1,600-2,800
	1,800-2,800
	1,800-2,800

	Electric motor power (peak)
	kW
	17
	17
	17

	Electric motor torque (peak)
	Nm
	205
	205
	205

	Dimensions and weigths

	Length/width/height
	mm
	4,766/1,820/1,438
	4,766/1,820/1,438
	4,766/1,820/1,438

	Wheelbase
	mm
	2,865
	2,865
	2,865

	Turning circle
	m
	11.07
	11.07
	11.45

	Track width front/rear
	mm
	1,582/1,594
	1,582/1,594
	1,582/1,594

	Luggage compartment capacity, VDA1
	l
	455
	455
	455

	Kerb weight/payload/
permissible gross mass
	kg
	1,805/545/2,350
	1,810/545/2,355
	1,850/550/2,400

	Tank capacity/reserve
	l
	66/7
	66/7
	66/7

	Permissible trailer load, unbraked, braked (at 12%)
	kg
	750/1,800
	750/1,800
	750/1,800

	Performance
	
	

	Acceleration 0–100 km/h
	s
	8.1
	7.1
	7.1

	Top speed
	km/h
	228
	240
	238

	Fuel consumption and emissions

	CO2 emissions combined2
	g/km
	131-116
	131-116
	136-118

	Energy consumption combined2
	l/100 km
	5.0-4.4
	5.0-4.4
	5.2-4.5

	CO2 class2
	
	D
	D
	E-D


	Prices


	Price (excl. VAT)3
	euros
	44,820
	48,270
	50,270

	Price (incl. VAT)4
	euros
	53,336
	57,441
	59,821




I nuovi modelli Mercedes-Benz Classe C Station Wagon

	Mercedes-Benz C-Class Estate with high-tech petrol engine 2x4 (RWD)


	
	
	C 200
	C 250
	C 300
	C 300 e

	Drive
	

	Cylinder arrangement/number
	
	I4
	I4
	I4
	I4

	Displacement
	cc
	1,999
	1,999
	1,999
	1,999

	Rated output
	kW/hp
	130/177
	160/218
	190/258
	160/218

	at
	rpm
	5,000-6,100
	5,000-6,100
	5,800-5,800
	5,000-6,100

	Rated torque 
	Nm
	250
	320
	400
	320

	at
	rpm
	1,400-4,000
	1,400-4,000
	2,000-3,200
	1,800-4,000

	Electric motor power (peak)
	kW
	17
	17
	17
	100

	Electric motor torque (peak)
	Nm
	205
	205
	205
	440

	Dimensions and weights

	Length/width/height
	mm
	4,766/1,820/1,455
	4,766/1,820/1,455
	4,766/1,820/1,455
	4,766/1,820/1,458

	Wheelbase
	mm
	2,865
	2,865
	2,865
	2,865

	Turning circle
	m
	11.07
	11.07
	11.07
	11.07

	Track width front/rear
	mm
	1,582/1,594
	1,582/1,594
	1,582/1,594
	1,579/1,583

	Luggage compartment capacity, VDA1
	l
	490-1,510
	490-1,510
	490-1,510
	360-1,375

	Kerb weight/payload/
permissible gross mass
	kg
	1,775/540/2,315
	1,785/540/2,325
	1,805/535/2,340
	2,145/510/2,655

	Tank capacity/reserve
	l
	66/7
	66/7
	66/7
	50/7

	Permissible trailer load, unbraked, braked (at 12%)
	kg
	750/1,800
	750/1,800
	750/1,800
	750/1,800

	Performance
	
	
	

	Acceleration 0–100 km/h
	s
	8.7
	7.5
	6.3
	6.0

	Top speed
	km/h
	228
	244
	250
	240




	Fuel consumption and emissions

	Energy consumption combined, weighted (*with discharged battery)/ energy consumption combined, weighted + fuel consumption combined, weighted2
	l/100 km/


kw/h
l/100 km
	7.0-6.4
	7.1-6.4
	7.1-6.5
	*7.7-6.9


16.0-15.2
+2.7-2.4

	CO2 emissions combined, weighted/ CO2 emissions discharged battery2
	g/km
	161-145
	161-145
	162-147
	61-55/
175-158

	CO2 class combined, weighted/ CO2 class discharged battery2
	
	F-E
	F-E
	F-E
	B/F

	Prices

	Price (excl. VAT)3
	euros
	42,345
	47,345
	51,955
	57,305

	Price (incl. VAT)4
	euros
	50,391
	56,341
	61,826
	68,193




	Mercedes-Benz C-Class Estate with high-tech petrol engine 4x4 (AWD)

	

	
	
	C 250 4MATIC 
	C 300 e 4MATIC
	C 400 e 4MATIC

	Drive
	
	

	Cylinder arrangement/number
	
	I4
	I4
	I4

	Displacement
	cc
	1,999
	1,999
	1,999

	Rated output
	kW/hp
	160/218
	160/218
	190/258

	at
	rpm
	5,000-6,100
	5,000-6,100
	5,800-5,800

	Rated torque 
	Nm
	320
	320
	400

	at
	rpm
	1,400-4,000
	1,800-4,000
	2,000-3,200

	Electric motor power (peak)
	kW
	17
	100
	100

	Electric motor torque (peak)
	Nm
	205
	440
	440

	Dimensions and weights

	Length/width/height
	mm
	4,766/1,820/1,455
	4,766/1,820/1,458
	4,766/1,820/1,458

	Wheelbase
	mm
	2,865
	2,865
	2,865

	Turning circle
	m
	11.45
	11.45
	11.45

	Track width front/rear
	mm
	1,582/1,594
	1,579/1,583
	1,579/1,583

	Luggage compartment capacity, VDA1
	l
	490-1,510
	360-1,375
	360-1,375

	Kerb weight/payload/
permissible gross mass
	kg
	1,840/535/2,375
	2,190/505/2,695
	2,190/505/2,695

	Tank capacity/reserve
	l
	66/7
	50/7
	50/7

	Permissible trailer load, unbraked, braked (at 12%)
	kg
	750/1,800
	750/1,800
	750/1,800

	Performance
	
	

	Acceleration 0–100 km/h
	s
	7.3
	6.2
	5.4

	Top speed
	km/h
	242
	240
	240

	Fuel consumption and emissions

	Energy consumption combined, weighted (*with discharged battery)/ energy consumption combined, weighted + fuel consumption combined, weighted2
	l/100 km/



kw/h/
l/100 km
	7.4-6.6
	7.9-7.0




16.6-16.1
+2.9-2.2
	7.9-7.0




16.6-16.1
+2.9-2.2

	CO2 emissions combined, weighted/ CO2 emissions discharged battery2
	g/km
	169-150
	66-51/
180-160
	66-51/
180-160

	CO2 class/ CO2 class discharged battery2
	
	F-E
	B/G-F
	B/G-F

	Prices

	Price (excl. VAT)3
	euros
	49,345
	59,305
	63,105

	Price (incl. VAT)4
	euros
	58,721
	70,573
	75,095




	Mercedes-Benz C-Class Estate with high-tech diesel engine


	
	
	C 200 d
	C 250 d
	C 250 d 4MATIC


	Drive
	
	


	Cylinder arrangement/number
	
	I4
	I4
	I4

	Displacement
	cc
	1,992
	1,992
	1,992

	Rated output
	kW/hp
	120/163
	147/200
	147/200

	at
	rpm
	3,200-4,400
	3,400-3,600
	3,400-3,600

	Rated torque 
	Nm
	380
	440
	440

	at
	rpm
	1,600-2,800
	1,800-2,800
	1,800-2,800

	Electric motor power (peak)
	kW
	17
	17
	17

	Electric motor torque (peak)
	Nm
	205
	205
	205

	Dimensions and weigths

	Length/width/height
	mm
	4,766/1,820/1,455
	4,766/1,820/1,455
	4,766/1,820/1,455

	Wheelbase
	mm
	2,865
	2,865
	2,865

	Turning circle
	m
	11.07
	11.07
	11.45

	Track width front/rear
	mm
	1,582/1,594
	1,582/1,594
	1,582/1,594

	Luggage compartment capacity, VDA1
	l
	490-1,510
	490-1,510
	490-1,510

	Kerb weight/payload/
permissible gross mass
	kg
	1,860/540/2,400
	1,860/540/2,400
	1,915/495/2,410

	Tank capacity/reserve
	l
	66/7
	66/7
	66/7

	Permissible trailer load, unbraked, braked (at 12%)
	kg
	750/1,800
	750/1,800
	750/1,800

	Performance
	
	

	Acceleration 0–100 km/h
	s
	8.3
	7.3
	7.3

	Top speed
	km/h
	224
	236
	234

	Fuel consumption and emissions

	Energy consumption combined2
	l/100 km
	5.1-4.6
	5.1-4.6
	5.4-4.7

	CO2 emissions combined2
	g/km
	134-120
	134-120
	141-123

	CO2 class2
	
	D
	D
	E-D


	Prices


	Price (excl. VAT)3
	euros
	46,120
	49,570
	51,570

	Price (incl. VAT)4
	euros
	54,883
	58,988
	61,368
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